 ------------------------------------------------------------------
 Morovia DataBar Scalable PCL fonts test sheet (I)

 Font used in test: mrvdatabar-34x.sft
 The bar height is 34X in the barcodes created. The font is ideal 
 for creating DataBar-14, DataBar Stacked Omnidirectional, DataBar Expanded
 and DataBar Expanded Stacked.
 
 After the font is downloaded into the printer, use 
 '<esc>(8U<esc>(s1p18v33218T' to select the font. Note that 18v sets the font
 size to 18 points. You can change to any optimal sizes that fit your printer.
 
 When producing stacked barcodes (DataBar Stacked Omnidirectional and 
 DataBar Expanded Stacked), you must set VMI properly. For this font (mrvdatabar-34x.sft)
 the VMI is font_size*1.48. If you use cursor movement, the cursove needs
 to move down font_size*0.0307 inch a row.
 ------------------------------------------------------------------
(3@

   12 points, DataBar-14:  (8U(s1p12v33218Ta1a3d2b2a1c3g1a4b2a2a2a1a2b1f1a1a7c3b2b1a3c2a1(3@
   
   
   12 points, DataBar Expanded: (8U(s1p12v33218Tamaammmaammaaaaamamammmmmmmmaaaamammmaaaammaamamaaammamaaaaaammaaamamammmmmmaaaammmamaammmaaaaaamaamamaammmmmammmaammaaammmmmmaaaamammamaaammaaammaaamamamaaaaaaaamaaamammmmmmmmaammmaaammammmmamaaaamam(3@
   



  16 points, DataBar Stacked Omnidirectional:
(8U(s1p16v33218T  
&l23.68C   
amammmamaamaaaaaamaammmaaaaaaaamamaaaamammmmmamama
mammnpsqsumvsurvspspmpmumumuntnpsprvrunvnpmpnvamam
(3@  
&l8C 

  16 points, DataBar Expanded Expanded: 
(8U(s1p16v33218T  
&l23.68C  
amaammmaammaaaaamamammmmmmmmaaaamammmaaaammaamamaaammamaaaaaammaaamamammmmmmaaaammmamaammmaaaaaamaamam
mamanqnuspmurvrunvnumpaqmpmprprpnunqnusvsqnvsqrqrvrqnvmusvsurqnvrvmunuaqaqmprprpnonumvspmpsururunvmama

(3@  
&l8C
